# Error ID codes

This table summarizes Error ID codes.

Word | ID code | Description
--- | --- | ---
0x0000 | No Error | No error occurred.
0x0100 | Trigger set while disabled | Occurs when the Trigger bit is set while the Trigger Enable bit is cleared and the AcquireImage function's Trigger parameter is set to External, Network or Industrial Ethernet.
0x0101 | Trigger set while Offline | Occurs when the Trigger bit is set while the vision system is Offline.
0x0400 | Already Executing Error | Occurs when the Execute Command bit is set and the Executing bit is still High.
0x0401 | Job load requested while Online | Occurs when a Job Load command is issued while the vision system is Online.
0x0402 | Job load requested does not exist on the camera | Occurs when a JobID sent in the Command field does not exist as a prefix for any job in the camera file system. For example, if you send Command = 123, but there is no job on the camera which contains 123xxxxx.job.