# HMI Filmstrip Properties

The HMI Filmstrip web page element has the following specific properties available in the Properties window when selected in the Web Page Editor:

Frequently Used properties:

- Delay to Continue: Specifies the interval (in milliseconds) that must pass after clicking the (Play) button to start queuing acquisitions again on the Filmstrip. The default value is 0, meaning that no delay will be used for queuing.
- Pause on Fail: Pauses the Online job in case a failed acquisition is recorded on the Filmstrip. This option is disabled by default.

- Task Name: Specifies the inspection whose acquisitions the HMI Filmstrip will display. Select InspectionTask from the drop-down list.

  Note: This property must be configured for the HMI Filmstrip to show recordings.

Display properties:

- Marker Style: Specifies the style of the Pass/Fail graphics used on the Filmstrip's inspection area. Use the drop-down menu to select the desired visual style. The default style is Sphere and Cube.
- Show Control Buttons: Shows or hides the control buttons of the Filmstrip, used to switch the Filmstrip between Live and Frozen modes, and navigate/save the acquisitions while in Frozen mode. This setting is checked by default, meaning that the control buttons are shown on the Filmstrip.
- Show Status Bar: Shows or hides the status bar at the top of the Filmstrip, used to provide an overall color-coded overview on the number of passed and failed acquisitions. This setting is checked by default, meaning that the status bar is shown on the Filmstrip.

Tip: Even if the Control Buttons and/or the Status Bar of the Filmstrip is disabled, you can still configure control and navigational buttons for the Filmstrip with the available Filmstrip click commands or $ functions.