# TransInspEdgeDefectToWorld

Applies a coordinate transform to an InspectEdgeForDefect data structure.

Note: The output of any vision tool that reports in real-world coordinates cannot be used as a fixture or region input to another vision tool.

## TransInspEdgeDefectToWorld Inputs

Parameter | Description
Calib | A reference to a spreadsheet cell containing a valid Calib data structure.
InspectEdgeForDefect | A reference to a spreadsheet cellcontaining a valid InspectEdgeForDefect data structure.

## TransInspEdgeDefectToWorld Outputs

Returns | InspectEdgeForDefect structure translated to world coordinates, or #ERR if any of the input parameters are invalid.