# About This Release

## New features

The In-Sight 3D 1.3.2 introduces the following new features and enhancements:

- Adding option to force Z axis on some of the 3D Fixture tools.

- Adding getScanTime getter to know the required time to acquire a Point Cloud. This getter only returns true values for real acquisitions, in case of working with filmstrips, this getter returns zero.

## Compatibility

3D-L4000 supports the following firmware versions:

- In-Sight Vision Suite 3D-L4000 1.0.0

- In-Sight Vision Suite 3D-L4000 1.0.1

- In-Sight Vision Suite 3D-L4000 1.2.0

- In-Sight Vision Suite 3D-L4000 1.3.0

- In-Sight Vision Suite 3D-L4000 1.3.2

You can install version 1.0.1, 1.2.0, 1.3.0, and 1.3.2 of 3D-L4000 In-Sight Vision Suite on the same computer at the same time. Upgrade and downgrade between 1.0.1, 1.2.0, 1.3.0 and 1.3.2 firmware versions is also possible.

Note: After upgrading from 1.0.0 to any other version, downgrading back to 1.0.0 is not possible.