# Time/Timer Vision Data Access Functions

This topic lists the Vision Data Access Functions that report execution cell times, read date and time from an internal clock, and trigger an event after a specified interval or at specified times.

Note: All returned values are from a referenced function or cell.

Function | Description
--- | ---
GetAllTime(Image) | Returns the time of a job execution in milliseconds. The returned value does not include the acquisition time. The function returns #ERR if the input value is invalid.
A | Acquisition ends.
B | Job execution ends.

To use GetAllTime:

1. Insert GetAllTime(A0) to a cell.

2. Trigger the In-Sight vision system.

   Note: The GetAllTime function calculates the time based on the last image acquisition. The return value of the function can be large at first. Make sure to trigger the vision system to get the correct value.
3. The time is returned to the cell.

Note:

- This argument must reference cell A0, the cell containing the Image data structure returned by the InputPointCloud function.
- You cannot use this function in a formula. For example, if you enter "GetAllTime(A0)+10" in a cell, #ERR is returned. To use a formula, create a separate cell just for GetAllTime(A0), and use a cell reference for it in the formula. For example, you can configure the spreadsheet as follows:
  - B2 = GetAllTime(A0)
  - B3 = B2+10