# Known Issues

Issue # | Known Issue
--- | ---
ISNG-10732 | In-Sight vision systems may not be able to load jobs outside of the In-Sight 3D adapter (for example by changing the running job with a PLC command, or setting the job as a startup job with the Startup Settings utility of In-Sight Vision Suite) if you create the new job by copying and then renaming the *.jobx file of another existing job. However, you can still load such jobs in the In-Sight 3D adapter. To ensure that the vision system can load your job as a startup job, or can switch to it with the available PLC job change commands, make sure that you always save your new job with the Save as option of the In-Sight 3D adapter.
N/A | The 3D-L4000 can stop responding to triggers when working with dual channel and encoder delay, and the motion is reversed such as in the case of stopping the belt. The workaround is to change to single channel. If the device is already field corrected, you can avoid repeating the correction process by unlocking the field correction and doubling the encoder resolution value. This is because the encoder resolution for single channel is half of the encoder resolution for dual channel.
ISNG-10588 | When saving a job whose filename and path are longer than 240 characters, the adapter throws a "Could not find a part of the path" Save Error exception. This error is due to the filename and path length limitations of Windows 10. To work around this problem, make sure that the path and filename combination of your job is shorter than 240 characters.
N/A | Occasionally, certain Job Windows of the In-Sight 3D development adapter may not appear on the GUI, even when using their View options in the menu bar to bring them forward. If you experience this problem, restore the workspace with the following steps to solve the issue: Open the Tools > Options menu of the Menu Bar. Navigate to the Workspace settings group of the Options window. Click the Reset Workspace button.