# EtherNet/IP Output Assembly - Instance 23

Note: For detailed descriptions of the signals, see Industrial Communications Signals.

Instance | Byte | Bit 7 | Bit 6 | Bit 5 | Bit 4 | Bit 3 | Bit 2 | Bit 1 | Bit 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
23 | 0 | Set Paused | Reserved | Execute Command | Inspection Results Acknowledge | Buffer Results Enable | Trigger | Trigger Enable
1 | Reserved
2 | Reserved | Clear Exposure Complete | Clear Error | Reserved | Set User Data
3 | External Event 7 | External Event 6 | External Event 5 | External Event 4 | External Event 3 | External Event 2 | External Event 1 | External Event 0
4 .. 5 | Command ID
6 .. 7 | Reserved
8 .. 495 | User Data 0 - 487