# Mapping of I/O Assembly Data Attribute Components

The following table indicates the I/O Assembly Data attribute mapping for In-Sight vision systems:

Data Component Name | Class | Instance Number | Attribute
--- | --- | --- | ---
Name | Number | Name | Number
Set Offline | Vision | 78 Hex | 1 | SetOffline | 8
Trigger Enable | Vision | 78 Hex | 1 | AcqTriggerEnable | 9
Trigger | Vision | 78 Hex | 1 | AcqTrigger | 10
Buffer Results Enable | Vision | 78 Hex | 1 | BufferResultsEnable | 13
Soft Event N | Vision | 78 Hex | 1 | SoftTrigger bit N | 18
Online | Vision | 78 Hex | 1 | Onlne | 6
Offline Reason | Vision | 78 Hex | 1 | OfflineReason | 7
Trigger Ready Trigger Ack Exposure Complete Missed Acquisition | Vision | 78 Hex | 1 | AcqStatusRegister | 11
User Data | Vision | 78 Hex | 1 | UserData | 12
System Busy Inspection Completed Results Buffer Overrun Results Valid | Vision | 78 Hex | 1 | InspectionStatusRegister | 14
Inspection ID Inspection Data | Vision | 78 Hex | 1 | InspectionResults | 16