# Updating the Job in the Adapter

Place the vision system Offline by either clicking the Sensor > Offline option, or clicking the Offline icon. Update the In-Sight Spreadsheet so that it contains a tool to generate data, a FormatOutputBuffer function that references the output of the tool, and a WriteResultsBuffer function that references the FormatOutputBuffer function. Then, place the vision system Online again by either clicking the Sensor > Online option, or clicking the Online icon.