# Setting up the In-Sight Vision System

The first step of configuring communication between an In-Sight vision system and the PLC is enabling PROFINET communication on the vision system. Perform the following steps to configure the vision system accordingly:

1. Launch In-Sight Vision Suite.

2. Click on the Utilities ribbon on the bottom of the page. The available utility icons appear.

3. Click on the Industrial Ethernet utility. The Industrial Ethernet configuration utility opens.

4. Select the PROFINET protocol from the drop-down list. Once selected, additional options appear in the window.

5. Check the Enable PROFINET Station Name option, then type ISVisionSystem in the Station Name textbox. Once finished, click OK.

Note: If the vision system was using a different Industrial Ethernet configuration prior to this change, the vision system must be restarted after clicking OK.