# In-Sight D900 Series Vision System Connection Requirements

The following are the recommended system requirements for connecting to an In-Sight D900 series vision system:

## Network Switch

- A Gigabit Ethernet network switch (managed or unmanaged) for connection to the In-Sight D900 series vision system.

## Power Supply

- For the In-Sight D900 series vision system, a power source rated for at least 5A continuous current is recommended.

CAUTION: The In-Sight Vision Suite and In-Sight ViDi software require that a valid Cognex Security Dongle be installed directly to PCs running the software during all phases of operation (programming, processing, training, testing, etc.). Any attempts to temporarily remove, substitute, or share a Cognex Security Dongle may cause your system to operate incorrectly, and may result in the loss of data.