# EtherNet/IP Input Assembly - Instance 11

Note: For detailed descriptions of the signals, see Industrial Communications Signals.

Instance | Byte | Bit 7 | Bit 6 | Bit 5 | Bit 4 | Bit 3 | Bit 2 | Bit 1 | Bit 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
11 | 0 | Online | Paused | Reserved | System Ready
1 | Error | Command Failed | Command Completed | Command Executing | Reserved
2..3 | Reserved
4..5 | Command Result Code
6..7 | Error ID
8..11 | External Event Acknowledge 0 - 31
12..15 | Reserved
16 | Results Buffer Overrun 0 | Inspection Passed 0 | Results Valid 0 | Inspection Completed 0 | Exposure Complete 0 | Acquisition Error 0 | Trigger Acknowledge Camera 0 | Trigger Ready Camera 0
17 | Reserved | Set User Data Acknowledge 0
18..19 | Acquisition ID 0
20..21 | Inspection Image ID 0
22..23 | Inspection Result Code 0
24 | Results Buffer Overrun 1 | Inspection Passed 1 | Results Valid 1 | Inspection Completed 1 | Exposure Complete 1 | Acquisition Error 1 | Trigger Acknowledge Camera 1 | Trigger Ready Camera 1
25 | Reserved | Set User Data Acknowledge 1
26..27 | Acquisition ID 1
28..29 | Inspection Image ID 1
30..31 | Inspection Result Code 1
32 | Results Buffer Overrun 2 | Inspection Passed 2 | Results Valid 2 | Inspection Completed 2 | Exposure Complete 2 | Acquisition Error 2 | Trigger Acknowledge Camera 2 | Trigger Ready Camera 2
33 | Reserved | Set User Data Acknowledge 2
34..35 | Acquisition ID 2
36..37 | Inspection Image ID 2
38..39 | Inspection Result Code 2
40 | Results Buffer Overrun 3 | Inspection Passed 3 | Results Valid 3 | Inspection Completed 3 | Exposure Complete 3 | Acquisition Error 3 | Trigger Acknowledge Camera 3 | Trigger Ready Camera 3
41 | Reserved | Set User Data Acknowledge 3
42..43 | Acquisition ID 3
44..45 | Inspection Image ID 3
46..47 | Inspection Result Code 3
48..499 | Inspection Results 0...451