# Configure Acquisition with AcquireImage

The AcquireImage function, in cell A0, defines the job's acquisition settings, and is used to configure the acquisition settings for the In-Sight D900 series vision system and its associated job. Every time a new image is acquired, the A0 cell containing AcquireImage, and all of its dependent cells, are executed.

Note:

- Please refer to the AcquireImage function topic for information about parameters and their settings. This topic is meant as an introduction to the function.
- The AcquireImage settings, however, can be overridden and/or adjusted through the use of one or more ApplyAcquisitionSettings functions.