# Setting up the In-Sight Vision System

The first step of configuring communication between the In-Sight vision system and the PLC unit is enabling PROFINET communication on the vision system. Perform the following steps to configure the vision system accordingly:

1. Launch In-Sight Vision Suite.

2. Click on the Utilities ribbon on the bottom of the page. The available utility icons appear.

3. Click on the Industrial Ethernet utility (marked below). The window of the Industrial Ethernet configuration utility opens.

4. Select the PROFINET protocol from the drop-down list. Once selected, additional options appear in the window.

5. Tick the Enable PROFINET Station Name option, then type isvc200 in the Station Name textbox. Once finished, click OK.

Note: In case the In-Sight vision system was using a different Industrial Ethernet configuration prior to this change, the vision system must be restarted after clicking OK.