# TransSurfaceFlawToWorld

Applies a coordinate transform to a SurfaceFlaw data structure.

Note: The output of any vision tool that reports in real-world coordinates cannot be used as a fixture or region input to another vision tool.

## TransSurfaceFlawToWorld Inputs

Parameter | Description
Calib | A reference to a spreadsheet cell containing a valid Calib data structure.
SurfaceFlaw | A reference to a spreadsheet cell containing a valid SurfaceFlaw data structure output by a SurfaceFlaw function.

## TransSurfaceFlawToWorld Outputs

Returns | A SurfaceFlaw data structure translated to world coordinates, or #ERR if any of the input parameters are invalid. Note: If Calibrate is used, all perimeter values will be returned in pixel coordinates. A flaw's roundedness and/or intensity values will not be converted to real-world values.