# Drag-and-Drop Communication Properties to Web Pages

You can quickly create WebPage Elements on a WebPage to display diagnostic information about the job's communication status while Online.

Just drag-and-drop the CommunicationCard tag from the Tags Window (published tags are in the Devices > CommunicationCard category) onto the WebPage.

When you drag-and-drop the tag, the following WebPage elements are automatically created:

WebPage Control Name | WebPage Control Text or Value | WebPage Label Text
IsConnected | True or False, depending on the connection status. | Same as Tag.
PLCConnectionUp | True or False, depending on the connection status. | Same as Tag.
ProtocolStatus | The code of the current protocol connection status. This can be one of the following: 4929: The connection is idle. 4930: The system is connecting. 4931: The system is connected. -2147478716: Connection rejected. -2147478715: Connection faulted. -2147478701: Connection timed out. -2147475295: The selected protocol is not enabled. | Same as Tag.