# Checking the Application

Once the job has been configured in the In-Sight ViDi adapter, the Online Enabled and Online Enable Comm bits should have a value of true in SIMATIC Manager while the job is running on the In-Sight vision system.

To trigger the In-Sight vision system, perform the following steps:

1. Enable the Trigger Enable bit. To do so, set this bit to true in the Modify value column, then click the Activate modify values icon. The Trigger Ready Cam0 bit then should become true, indicating that the vision system is ready to be triggered.

2. Trigger the vision system by giving it a rising edge on Trigger Cam0. “Rising edge” means that the bit is first set to true (by setting it to true in the Modify value row and clicking on the Activate modify values icon), and then set back to false.

   When the bit is set to true, the Trigger Ack Cam0 and Exposure Complete Cam0 bits should also change to true, indicating that triggering is completed. The Acquisition ID Cam0 value is incremented each time the camera is triggered.

   Likewise, once Trigger Cam0 is set back to false, the Trigger Ack Cam0 bit also changes to false again.

3. Check the job; the newly-acquired image should appear.