# FindCurve

Locates a single circular arc edge segment within a curved image region. FindCurve forms a one-dimensional projection of the image region by summing pixel values on concentric arc segments scanned in the positive x-direction relative to the region's local coordinate system. Edge transitions are extracted from the projected image data.

## FindCurve Inputs

Parameter | Description
Image | This parameter must reference a spreadsheet cell that contains an Image data structure; by default, this parameter references A0, the cell containing the AcquireImage data structure. This parameter can also reference other Image data structures, such as those returned by the Image Vision Data Access Functions or Coordinate Transforms Functions.
Fixture | Defines the Region of Interest (ROI) relative to a Fixture input or the output of a Vision Tools function's image coordinate system. Setting the ROI relative to a Fixture ensures that if the Fixture is rotated or translated, the ROI will be rotated or translated in relation to the Fixture. The default setting is (0,0,0), the top leftmost corner of the image.
X | The X offset, in image coordinates.
Y | The Y offset, in image coordinates.
Theta | The rotation from the image X axis, in the image coordinate system. (+/-360 degrees clockwise)
Region | Also known as the Region of Interest (ROI), specifies the region of the image that undergoes analysis; creates an Interactive Graphics Mode that can be transformed and rotated. With this parameter selected, by pressing the Maximize Region button on the property sheet's Job Edit toolbar, the region will automatically be stretched to cover the entire image.
X | The x-offset of the origin, in fixture coordinates.
Y | The y-offset of the origin, in fixture coordinates.
Width | The dimension along the region's x-axis.
Height | The dimension along the region's y-axis.
Angle | The orientation, in fixture coordinates.
Curve | The angular deviation between the region's x-axis and the opposing boundary line.
Note: The Fixture and Region parameters must be defined within the bounds of the image; otherwise, the function will return #ERR.
Polarity | Specifies the polarity of the edge to be located, relative to the scan direction of the Edge Region; the function will only report edges of the specified polarity.
0 = black-to-white | Specifies that the edge polarity is black-to-white.
1 = white-to-black | Specifies that the edge polarity is white-to-black.
2 = either (default) | Specifies that the edge polarity could be either black-to-white or white-to-black.
Find By | Specifies the edge selection technique the function will use to select an edge, amongst multiple edge candidates.
0 = best score (default) | Specifies that the edge with the highest score receives the highest consideration.
1 = first edge | Specifies that the first edge detected receives the highest consideration.
2 = last edge | Specifies that the last edge detected receives the highest consideration.
Accept Thresh | Specifies the minimum acceptable edge contrast (0 to 100; default = 25); the contrast value is normalized from the greyscale histogram within the Region to a scale of 0 to 100. The function will reject any edge whose contrast score falls below this value.
Normalize Score | Specifies whether the edge scores will be normalized by the greyscale histogram of the Region. When Normalize Score is enabled, raw edge scores are normalized by the maximum contrast found within the image region using the following formula: Score = (Raw Edge Score) x (100/Max Contrast) Where Raw Edge Score is the grey level difference across the edge and Max Contrast is the difference between the maximum and minimum grey level (0 to 255) within the image region. When Normalize Score is disabled, low contrast edges will score lower than high contrast edges. The following formula is used: Score = (Raw Edge Score) x (100/255)
0 = OFF | Do not normalize the score.
1 = ON (default) | Normalize the score.
Tip: This parameter is useful for finding edges in a low contrast region. If the edges to be detected are expected to be only high contrast, disable this parameter.
Angle Range | Specifies the function's tolerance to edge rotation (0 to 10; default = 0). The function will still find edges that are outside of the specified range, but the accuracy may not be as high. Note: Setting this parameter to a value greater than 0 will reduce the speed of the function. This setting is currently ignored; the maximum Angle Range of 10 is always allowed within an annular segment.
Edge Width | Specifies the pixel distance (1 to 50; default = 3) over which an edge transition takes place. Edge Width is used to filter the image before edges are extracted.
Show | Specifies the display mode for FindCurve graphical overlays on top of the image.
0 = hide all (default) | All graphics will be hidden, except when the cell containing the FindCurve function is the active cell in the spreadsheet.
1 = result graphics only | The curved edge will be displayed at all times.
2 = input and result graphics | Both the input image region and the curved edge will be displayed at all times.
3 = show all: input, result, and chart | The input image region, the curved edge, and the edge response chart will be displayed at all times. Note: The edge response chart is a dockable window. For more information, see the Spreadsheet Editor – Charts topic.

## FindCurve Outputs

Returns | An Edge data structure containing a single curved edge segment, or #ERR if any of the input parameters are invalid.
Results | When FindCurve is initially inserted into a cell, a result table is created in the spreadsheet. The following Edges Vision Data Access Functions are automatically inserted into the spreadsheet to create the result table:
CentX | GetX(Edges, 0, 0) | The x-coordinate of the center of curvature.
CentY | GetY(Edges, 0, 0) | The y-coordinate of the center of curvature.
StartX | GetX(Edges, 0, 1) | The x-coordinate of the first endpoint.
StartY | GetY(Edges, 0, 1) | The y-coordinate of the first endpoint.
EndX | GetX(Edges, 0, 2) | The x-coordinate of the second endpoint.
EndY | GetY(Edges, 0, 2) | The y-coordinate of the second endpoint.
Radius | GetRadius(Edges, 0) | The arc radius.
Score | GetScore(Edges, 0) | The edge contrast score. Score is positive for black-to-white transitions, negative for white-to-black transitions.