The following table describes the trigger settings available on the Image panel:

Setting | Description
--- | ---
Trigger Type | Defines the type of trigger signal that begins an image acquisition Acquisition is the process or result of the vision system acquiring a new image.. The following options are available: Single: An external trigger event triggers the start of an acquisition and an inspection. Self: Acquisitions and inspections occur periodically.
Trigger Interval (ms) | Defines the time in milliseconds between acquisitions when Self trigger type is selected. The available values are 0–10000. Note: Appears only when Trigger Type is set to Self.
Trigger Source | Defines the trigger source for the acquisition. The following trigger sources are available: Trigger Input Line: Trigger acquisition when the trigger input of the vision system line goes high. Camera Trigger Button: Trigger acquisition by pressing the trigger button on the vision system. Native Mode: Trigger acquisition by sending a Native Mode command to the vision system. Network (UDP): Trigger acquisition when the vision system receives a specifically formatted UDP package. Factory Protocols: Trigger acquisition by toggling a bit with the configured industrial protocol. WebHMI The operator interface through which the operator interacts with the vision system. Trigger Button: Trigger acquisition by pressing the trigger button in the WebHMI. Note: Appears only when Trigger Type is set to Single.
Debounce (ms) | Defines the time in milliseconds that a trigger has to last to trigger an acquisition. The available values are 0–10. Note: Appears only when Trigger Type is set to Single.
Delay (ms) | Defines the delay between the time that the vision system receives a trigger to acquire an image, and the time the vision system begins the image acquisition. The available values are 0–10000. Note: Appears only when Trigger Type is set to Single.