The following table describes the illumination settings available on the Image panel:

Setting | Description
--- | ---
Mode | Defines the illumination device. The following options are available: Disabled Integrated Illumination External Illumination
Intensity | Specifies the intensity of the illumination device. The available values are 0–100.
Always On | When enabled, the illumination device is on continuously. The following options are available: Disabled Enabled
Strobe Start | Defines when the strobe fires. The following options are available: Camera Trigger Acquisition Acquisition is the process or result of the vision system acquiring a new image. Start Note: Appears only when Mode is set to External Illumination.
Strobe Polarity | Defines the signal that fires a connected strobe. The following options are available: Low High Note: Appears only when Mode is set to External Illumination.
Banks Enabled | Check or uncheck the checkboxes inside the banks on the graphic to enable or disable each bank. Banks graphics can vary depending on the illumination hardware attached to the vision system. Note: Appears only when Mode is set to Integrated Illumination.
Light Color | Defines the color of the illumination. The following options are available: WHITE RED GREEN BLUE Note: Appears only when Mode is set to Integrated Illumination.