The following table describes the image size settings available on the Image panel:

Setting | Description
--- | ---
Start Row | Defines the first row to transfer from the image sensor into the memory of the vision system. The available values are 0–1079. Note: For IS2800, ADV182, and IS3800 models, values must be divisible by 4.
Number of Rows | Defines the number of image sensor rows to transfer into the memory of the vision system. The available values are 4–1080. Note: For IS2800, ADV182, and IS3800 models, values must be divisible by 4.