# Acquisition Duration

Specifies when to end image acquisition Acquisition is the process or result of the vision system acquiring a new image. if the Clip Mode is set to Fill Black or Reduce Image.

The following options are available:

- Next Trigger (default): Image acquisition begins at the leading edge of the trigger pulse and ends at the beginning of the next trigger signal.

- End of Trigger: Image acquisition begins at the leading edge of the trigger pulse and ends at the trailing edge of the trigger pulse. Image acquisition is complete when one of the following occurs:

  - The specified Number of Lines have been acquired, even if the trailing edge of the trigger pulse has not yet arrived.

  - The trailing edge of the pulse arrives and terminates acquisition before the specified Number of Lines have been acquired.

Note: The End of Trigger mode can only be used with the Reduce Image clip mode.