# Enterprise Connectivity Metrics

The Enterprise Connectivity Metrics dialog allows you to add named cells for forwarding metrics through an MQTT Message Queue Telemetry Transport (MQTT) is a lightweight messaging protocol used to send and receive data between devices. connection.

To add a named cell to the list of metrics, click the + button in the top right of the dialog, and select the named cell that you want to add from the dropdown menu that appears.

Note: You can only add named cells to the list of metrics. If you do not have any named cells in your Spreadsheet job A job is a user-configured program in In-Sight Spreadsheet consisting of functions and designed for specific applications. You can create and edit jobs using the In-Sight Spreadsheet interface, and load them on a vision system for deployment in a live environment., no options appear when you try to add metrics.

You can configure the following additional parameters for the added metrics:

Parameter | Description
--- | ---
Metric ID | The ID for the metric A metric is a data value with additional context such as type or properties that explain what the value means and how it is used or shown, helping systems understand and work with the data correctly. in the MQTT message.
Metric Type | The type of the metric: Text Classification Counter Identification Measurement
Metric Value | The value of the metric, which is defined by the value in the named cell.
Edit Metric Details | Click the Edit Metric Details button to add a description for the metric.