# Acquisition Timeout

Defines the maximum amount of time to acquire an image in milliseconds. If the vision system does not complete image acquisition Acquisition is the process or result of the vision system acquiring a new image. within the specified time, the vision system aborts the acquisition and an issues Acquisition Error.

The available values are 0–10000. The default value 0 means that the timeout is disabled.