# TransEdgesToFixture

Converts an Edge structure from image coordinates to fixture A fixture is a coordinate location on the image that keeps the tool in the place determined by the fixture. coordinates. The function Functions are tools that are available in Spreadsheet for processing and analyzing acquisitions or other results. You can add functions to your Spreadsheet job to create tool chains and produce results for specific applications. computes the offset and orientation of the edges with respect to the specified fixture.

Inputs

The TransEdgesToFixture function has the following syntax:

TransEdgesToFixture(X, Y, Theta, Edges, Number to Convert)

See the table for a description of the available parameters.

Parameter | Description
Fixture | Specifies the fixture coordinate system.
X | Offset from image X-origin.
Y | Offset from image Y origin.
Theta | The rotation from the image X-axis, in the image coordinate system. (+/-360 degrees clockwise)
Edges | This argument must reference a spreadsheet cell that contains a valid Edges data structure.
Number to Convert | Number of edges to convert to real-world coordinates between 0 and 2591. The default number is three.

Outputs

Returns | An Edges data structure containing the transformed edges, or #ERR if any of the input parameters are invalid.
Results | When the function is initially inserted into a cell, a result table is created in the spreadsheet.

Vision Data Access functions

The Edges Vision Data Access functions automatically inserted into the spreadsheet is similar to those automatically inserted by the functions used for SortEdges and PairEdges data structures.