# SLMP PLC Configuration

The In-Sight Spreadsheet vision system supports SLMP, a common protocol establishing seamless connection between CC-Link IE and TCP/IP-based products. This protocol is used by the application to communicate with Mitsubishi iQ-Q and FX Series PLCs/Motion Controllers (MCs) installed on the network. Compared to the EtherNet/IP and PROFINET-based network communications (where the input and output communication is controlled by the PLC A Programmable Logic Controller is a ruggedized computer that you can use for automating processes or even an entire production line./MC), SLMP communication between In-Sight Spreadsheet vision system and the PLC/MC is initiated by the vision system.

Follow the below steps to enable the SLMP protocol for In-Sight Spreadsheet vision system:

1. Launch In-Sight Vision Suite, and open the Industrial Ethernet utility from the Utilities window.
2. Select SLMP from the dropdown list. The protocol-specific Settings and Device Addressing tabs then appear. Configure the connection according to the local network properties.
3. Install the GX Works application on the same PC as In-Sight Vision Suite. Download the application from Mitsubishi Electric Factory Automation downloads.
4. Launch the GX Works application and configure the In-Sight vision system so that it can communicate with the Mitsubishi PLC/MC. For more information, see the GX Works Operating Manual.