# In-Sight 3800 Utilities

Utility Button | Utility Name | Description
--- | --- | ---
| Firmware Update | The Firmware Update utility helps you through the firmware update process. For more information, see Firmware Update.
| Restart | The Restart utility remotely restarts an In-Sight vision system. For more information, see Restart.
| Backup | The Backup utility backs up the selected vision system(s). For more information, see Backup.
| Restore | The Restore utility restores the selected In-Sight vision system. For more information, see Restore.
| User Settings | The User Settings utility allows you to configure users and their access capabilities on an In-Sight vision system. For more information, see User Settings.
| Industrial Ethernet | The Industrial Ethernet utility selects and configures an Industrial Communications protocol for the vision system. For more information, see Industrial Ethernet.
| Camera Configuration | The Camera Configuration utility allows you to configure the resolution for the vision system. For more information, see Camera Configuration.
| Go Offline | The Go Offline utility sets an Online job Offline on an In-Sight vision system. For more information, see Go Offline.
| File Management | The File Management utility allows you to view, copy, move, or delete files on the In-Sight vision system. For more information, see File Management.
| Startup Settings | The Startup Settings utility configures a startup job for the In-Sight vision system. For more information, see Startup Settings.
| License Configuration | The License Configuration utility updates the existing product license of your In-Sight vision system on the Cognex Security Dongle. For more information, see License Configuration.
| Network Settings | The Network Settings utility configures the network settings of an In-Sight vision system. For more information, see Network Settings.
| Time Settings | The Time Settings utility is used to configure the date and time settings of an In-Sight vision system. For more information, see Time Settings.
| Password Reset | The Password Reset utility resets the password of the default admin user on the selected In-Sight vision system(s). For more information, see Password Reset.
| Factory Reset | The Factory Reset utility restores an In-Sight vision system to its factory default settings. For more information, see Factory Reset.
| HMI Settings | The HMI Settings utility allows you to configure the HMI window. For more information, see HMI Settings.
| Calibration Grid | The Calibration Grid utility prints out a calibration grid paper to assist in calibrating between pixel and real-world coordinates. For more information, see Calibration Grid.
| Support Feedback | The Support Feedback utility (also known as the Report a Problem utility) prepares error reports for potential issues. For more information, see Support Feedback.
| Serial Configuration | The Serial Configuration utility allows you to configure the serial port of the vision system. For more information, see Serial Configuration.