# FindLine

Locates a single straight-line edge within an image region. FindLine forms a one-dimensional projection of the image region by summing pixel values on radial line segments scanned in the positive y-direction relative to the local coordinate system of the region. Edge transitions are extracted from the projected image data.

## FindLine Inputs

Parameter | Description
Image | This parameter must reference a spreadsheet cell that contains an Image data structure. By default, this parameter references A0, the cell containing the data structure. This parameter can also reference other Image data structures, such as those returned by the Image Vision Data Access functions or Coordinate Transforms Functions.
Fixture | Defines the Region of Interest (ROI) relative to a Fixture input or the output of the image coordinate system for the Vision Tools function. Setting the ROI relative to a Fixture ensures that if the Fixture is rotated or translated, the ROI is rotated or translated in relation to the Fixture. Note: 2D projections use real world units but fixturing with 2D tools requires input in pixel values. When using a 2D projection from a 3D point cloud as a Fixture, convert the real world units to pixel values using the TransWorldToPixel function. The default setting is (0,0,0), the top leftmost corner of the image.
X | The X-offset, in image coordinates.
Y | The Y-offset, in image coordinates.
Theta | The rotation from the image X-axis, in the image coordinate system. (+/-360 degrees clockwise)
Region | Also known as the Region of Interest (ROI), specifies the region of the image that undergoes analysis. Double-click on the Region parameter to create an Interactive Graphics Mode that you can transform and rotate. Select this parameter and press the Maximize Region button on the Job Edit toolbar of the property sheet to automatically stretch the region to cover the entire image.
X | The X-offset of the origin, in fixture coordinates.
Y | The Y-offset of the origin, in fixture coordinates.
Width | The dimension along the X-axis of the region.
Height | The dimension along the Y-axis of the region.
Angle | The orientation, in fixture coordinates.
Curve | The angular deviation between the x-axis and the opposing boundary line of the region.
Note: The Fixture and Region parameters must be defined within the bounds of the image. Otherwise, the function returns #ERR.
Polarity | Specifies the polarity of the edge to be located, relative to the scan direction of the Edge Region. The function only reports edges of the specified polarity. Note: When using a horizontal or vertical linear edge feature as a fixture input, the function will only account for the movement of the edge in one direction, either along the horizontal or vertical axis, depending on the position of the scan direction of the ROI.
0 = black-to-white | Specifies that the edge polarity is black-to-white.
1 = white-to-black | Specifies that the edge polarity is white-to-black.
2 = either (default) | Specifies that the edge polarity could be either black-to-white or white-to-black.
Find By | Specifies the edge selection technique the function uses to select an edge, amongst multiple edge candidates.
0 = best score (default) | Specifies that the edge with the highest score receives the highest consideration.
1 = first edge | Specifies that the first edge detected receives the highest consideration.
2 = last edge | Specifies that the last edge detected receives the highest consideration.
Accept Thresh | Specifies the minimum acceptable edge contrast (0 to 100; default = 25); the contrast value is normalized from the greyscale histogram within the Region to a scale of 0 to 100. The function rejects any edge whose contrast score falls below this value.
Normalize Score | Specifies whether the edge scores will be normalized by the greyscale histogram of the Region. When Normalize Score is enabled, raw edge scores are normalized by the maximum contrast found within the image region using the following formula: Score = (Raw Edge Score) x (100/Max Contrast) Where Raw Edge Score is the grey level difference across the edge and Max Contrast is the difference between the maximum and minimum grey level (0 to 255) within the image region. When Normalize Score is disabled, low contrast edges will score lower than high contrast edges. The following formula is used: Score = (Raw Edge Score) x (100/255)
0 = OFF | Do not normalize the score.
1 = ON (default) | Normalize the score.
Tip: This parameter is useful for finding edges in a low contrast region. If the edges to be detected are expected to be only high contrast, disable this parameter.
Angle Range | Specifies the tolerance of the function to edge rotation (0 to 10; default = 0). The function still finds edges that are outside of the specified range, but the accuracy may not be as high. Note: Setting this parameter to a value greater than 0 reduces the speed of the function.
Edge Width | Specifies the pixel distance (1 to 50; default = 3) over which an edge transition takes place. Edge Width is used to filter the image before edges are extracted.
Show | Specifies the display mode for FindLine graphical overlays on top of the image.
0 = hide all (default) | All graphics are hidden, except when the cell containing the FindLine function is the active cell in the spreadsheet.
1 = result graphics only | The line edge is displayed at all times.
2 = input and result graphics | Both the input image region and the line edge are displayed at all times.
3 = show all: input, result, and chart | The input image region, the line edge, and the edge response chart are displayed at all times.

## FindLine Outputs

Returns | An Edge data structure containing a single straight-line edge segment, or #ERR if any of the input parameters are invalid.
Results | When FindLine is initially inserted into a cell, a result table is created in the spreadsheet. The following Vision Data Access functions are automatically inserted into the spreadsheet to create the result table:
Label | Function | Description
--- | --- | ---
X0 | GetX(Edges,0,0) | The row coordinate of the first endpoint.
Y0 | GetY(Edges,0,0) | The column coordinate of the first endpoint.
X1 | GetX(Edges,0,1) | The row coordinate of the second endpoint.
Y1 | GetY(Edges,0,1) | The column coordinate of the second endpoint.
Score | GetScore(Edges,0) | The edge contrast score. Score is positive for black-to-white transitions, negative for white-to-black transitions.