# LIGHT.DIRECT

Please note, that this command is deprecated. It is recommended to use LIGHT.BANKS command as an alternative with the same functionality. Turns on/off light banks for the 8072V. Verification should only take place with lighting combinations that can be described as 30 single, 30T (opposite sides), 30Q (all 30 panels), 45Q (all 45 panels), or 90. Other lighting combinations are allowed by the firmware, but will not result in valid verification result.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
state | bool |  |

## Platforms

DM8072 Verifier

## Notes

Version: 5.7.7