View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# Can I send images to an FTP server?

Use the FTP Image tab to configure the settings necessary to transfer images to an FTP server. The tab contains settings for the IP address and port number of the server as well as a username and password combination. Be aware that images sent using FTP are not guaranteed to be sent, which can happen when the reader is operating at a higher frequency and cannot schedule time for transfer of images.

The File Name options allow you to specify the file where the images will be stored. The File Name field allows you to specify a path in relation to the FTP server's root directory (for example, /failed_images/image). The filename extension (.jpg or .bmp) presented in the label following the file name matches the image format setting on the Buffered Image Settings pane. Be aware that the reader does not create directories; the directory must be available and accessible.

The Max Append Value control indicates the limit of the increment value used in the file name. A value of 0 indicates that no increment will be appended and the file can be overwritten.

The Server Generated File Name option starts with a blank path, which indicates the root directory of the FTP server.

The What Images to Transfer list allows you to choose which type of images are sent to the FTP server. Be aware that the FTP server needs to support image transfer.

Note: DMAE50,DM060,DM070,DM200