View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What is DoD UID Validation?

DoD UID Validation is used to evaluate whether the data encoded in a Data Matrix code is encoded correctly according to the US Department of Defense's Mil Standard 130 guidelines. The US Department of Defense now requires all items (over $5,000 or that are uniquely serialized) that it receives or maintains in inventory be marked with a unique serial number (UII) and with a specific syntax format. The DoD UID Validation tool is used to confirm if the data in a code is formatted correctly according to the Department of Defense Construct types 1 or 2. The DoD UID Validation feature also automatically confirms if the data string correctly conforms to ISO 15434 and ISO 15418. The output of the Concatenated UII (or just the Data Elements of the UII without the ISO 15434 syntax and ISO 15418 data qualifiers) is displayed in the first results field in the Validation Results field in the Results Task Pane.

Construct 1 data elements include: The manufacturer's Enterprise Identifier EID (CAGE, DUNS, EAN.UCC) identifier for a company plus the serial number of the part within their EID identifier. The Enterprise Identifier and serial numbers are represented by specific Data Qualifiers depending on whether a company is using a DI, AI or TEI format.

Construct 2 data elements include: The manufacturer's Enterprise Identifier (EID), the manufacturer's part number (PN) and batch number (BN) identifier for the part and the unique serial number for the part within the manufacturer's specific part number. The Enterprise Identifier, part number/batch number and serial numbers are represented by specific Data Qualifiers depending on whether a company is using a DI, AI or TEI format.

Note: This option is not available on all readers.

Note: default,DMAE50,DM050,DM060,DM070,DM150,DM260,DM300,DM360, DM370,DM280, DM470, DM503,DM7500,DM8050,DM8070,DM8600,DM8700,MX-1000,MX-1500,DM9500