# EtherNet/IP Output Assembly - Instance 22

Instance | Byte | Bit 7 | Bit 6 | Bit 5 | Bit 4 | Bit 3 | Bit 2 | Bit 1 | Bit 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
22 | 0 |  |  |  | Execute Command | Inspection ResultsAck | Reserved | Trigger |
1 |
2 |  |  | Clear Error |  |
3 |  |  |  |  |  |  |  |
4 .. 5 | Command ID
6 .. 7 |

Copyright © 2023 | Cognex Corporation | All Rights Reserved.

In-Sight SnAPP Software Manual | 2024 February 21 | Revision: 23.1.0.16