# Secure Communication

Set up a secure communication channel between the vision sensor and the browser by uploading and using an SSL certificate.

The Applied SSL Certificate shows you which SSL certificate you are currently using.

To upload an SSL certificate, click on the Upload button and select the following files from your computer:

- Server Certificate

- Intermediate Certificate (optional)

- Certificate Key

The Status shows the statuses of the uploaded files.

Click on Upload Certificate to upload the chosen files.

Note: If you delete your certificate, your connection is no longer secure. In this case, you need to manually remove the "s" from the protocol in the URL to reconnect to the vision sensor.