# Ethernet/IP PLC Configuration

To configure Ethernet/IP:

1. Navigate to the Communications tab of the Settings menu.

2. Enable the Inputs and Outputs toggles.

3. Click on the Ethernet/IP button.

4. Click Apply.

For more information, see Communications.

Note: For more information about configuring Ethernet/IP with PLC, see the training videos on https://www.cognex.com/in-sight-snapp-support.