# Ensamblado de entrada EtherNet/IP - Instancia 13

Instancia | Byte | Bit 7 | Bit 6 | Bit 5 | Bit 4 | Bit 3 | Bit 2 | Bit 1 | Bit 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
13 | 0 | Online |  | Acq Error |  | Trigger Ack | Trigger Ready
1 | Error | Command Failed | Command Completed | Command Executing | Results Valid |  | Inspection Completed | Reserved
2 |  |  | InspectionPass |  |  |
3 |  |  |  |  |  |  |  |
4 .. 5 | Error ID (entero de 16 bits)
6 .. 7 |
8 .. 9 | Current Program ID (entero de 16 bits)
10 .. 11 | Acquisition ID (entero de 16 bits)
12 .. 13 | Inspection ID (entero de 16 bits)
14.. 15 |
16 .. 499 | Inspection Results 0 - 483

Nota: Para más información sobre los resultados de la inspección, véase Resultados de inspección.