# Tabla de referencia del módulo PROFINET

Módulo | ID | Byte | Bit 7 | Bit 6 | Bit 5 | Bit 4 | Bit 3 | Bit 2 | Bit 1 | Bit 0
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Acquisition Control | 0x101 | 0 |  |  |  | Trigger |
Acquisition Status | 0x201 | 0 | Online |  | Acquisition Error |  | Trigger Acknowledge | Trigger Ready
1 |
2..3 | Acquisition ID
Inspection Control | 0x102 | 0 | Clear Error |  | Execute Command |  | Inspection Results Acknowledge |
Inspection Status | 0x203 | 0 |  | Command Failed | Command Completed | Command Executing | Results Valid |  | Inspection Completed |
1 | Error |  | Inspection Passed
2..3 | Error ID
Command Control Input | 0x108 | 0..1 | Command ID (16-bit)
Command Control Output | 0x108 | 0..1 | Current Program ID (16-bit)
2..3 |
Inspection Results | 0x401 (16) 0x402 (32) 0x403 (64) 0x404 (128) 0x405 (250) | 0..1 | Inspection ID
2..3 |
4..253 máx. | Inspection Results

Nota: Para más información sobre los resultados de la inspección, véase Resultados de inspección.