# TCP/IP Settings

In the TCP/IP settings, you can edit the trigger command.

The Trigger Command is a string that the vision sensor receives through the TCP/IP communication channel and causes the vision sensor to trigger and capture a new image.

To edit the Trigger Command:

1. Choose a format. You can choose between HEX and Plaintext.

2. Write the new trigger command into the field.

3. Click Apply.

Note:

Before clicking Apply, you can use the Revert button to decline your changes.