# Ethernet/IP PLC Configuration

To configure Ethernet/IP:

1. Install and configure the PLC-specific files and software on the PC.

2. Verify that the PLC protocol is enabled and that the vision sensor appears in the software used to configure the PLC.

3. Connect to the vision sensor.

4. Go to the Communications tab of the Settings menu.

5. Enable the Inputs and Outputs toggles.

6. Click on the Ethernet/IP button.

7. Click Apply.

For more information, see Communications.

Note: For more information about configuring Ethernet/IP with PLC, see the training videos on https://www.cognex.com/in-sight-snapp-support.