# SLMP Cyclic Time and Data Sizes

SLMP supports cyclic connection times (or poll intervals) between 5–30000 ms.

The user data and the inspection result size within a cyclic connection depends on the type of the PLC/MC:

PLC Type | Bit/Word | Max Size (Bits)
Mitsubishi FX Series | bit | 256
word | 1024 (64 words)
Mitsubishi iQ-F Series | bit | 3584
word | 15360 (960 words)
Mitsubishi R/Q/L Series | bit | 3584
word | 15360 (960 words)
Mitsubishi CRD Robot Series | bit | N/A
word | 15360 (960 words)