# PROFINET PLC Configuration

To configure PROFINET:

1. Install and configure the PLC-specific files and software on the PC.

2. Verify that the PLC protocol is enabled and that the vision sensor appears in the software used to configure the PLC.

3. Connect to the vision sensor.

4. Go to the Communications tab of the Settings menu.

5. Enable the Inputs and Outputs toggles.

6. Click on the PROFINET button.

7. Fill in the fields.

8. Click Apply.

For more information, see Profinet Communications Settings.

Note: For more information about configuring PROFINET with PLC, see the training videos on https://www.cognex.com/in-sight-snapp-support.