# Dynamic Test

The Dynamic Test page of the EI Tunnel Manager Setup allows you to to perform a dynamic test of the tunnel in seven steps.

To set Set up the target box and perform dynamic tests:

1. Locate the box and the sheet of adhesive 1D and 2D code labels.

   Build the box and adjust the height to the maximum height supported by the tunnel.

   If 2D codes are in the dynamic test, apply the 2D codes from the label sheet to the box.

   Select the Include 2D Codes checkbox. This step is optional.

   Apply each code label within the corresponding rectangular outline printed on the target box by matching the first two characters of the code content and the two characters printed within the rectangle.

   Make sure you apply the label within the rectangle printed on the box as demonstrated below:

   Fill in the Test Parameters fields such as Test Case* and Box Height* and select an MRS group from the Primary Device list discovered by clicking on Discover Devices.

2. After seeing the message Device prepared successfully. Continue to the next step to begin the dynamic test., to create device backups and reconfigure all devices in the selected MRS group for the tests in the Device Preparation step, click on Next Step.

3. The Encoder Check step is the third one, allowing you to check if each device is receiving an encoder signal. To see the results, bring the conveyor belt up to full production speed and run a box through the tunnel. Any orientation is acceptable.

   After the encoder check is complete, you see the message All devices passed the encoder check. The right and left justified test steps are now available. and pass icons under the Pass column.

   To complete this step and switch to the Right-Justified Test step, click on Next Step.

4. In the Right-Justified Test step the right-justified test becomes active. For this test, run the test box right justified on the belt. Place the box on the belt with the front side facing downstream. Make sure to use the dynamic test box.

   Wherever possible, include box that runs at both slower (less than or equal to 300 ft/min or 1.52 m/s) and faster belt speed (greater than 300 ft/min or 1.52 m/s) before completing the test and generating the report.

   To make sure the box stays level to the belt, add weight to the box. Give the box enough distance before the tunnel, so it moves through at full speed.

5. To see the passed test details, click on the test row.

   More detailed test results open up.

   Review the table and verify there are no codes with an X. The X indicates that the code must be read but it was not read.

   The barcodes with the green check mark indicate that they must be read and were read successfully.

   - At belt speeds of less than 300 fpm we need every code to be read at least once.

   - At faster belt speeds each code needs to be read by the specific banks.

   It is possible that you have to run the box through multiple times to pass. Once you pass on all barcodes, you can move on to the Left-Justified Test step by clicking on Next Step.

6. In the Left-Justified Test step the left-justified test becomes active. For this test, run the test box right justified on the belt. Place the box on the belt with the front side facing downstream. Make sure to use the dynamic test box.

   Wherever possible, include box that runs at both slower (less than or equal to 300 ft/min or 1.52 m/s) and faster belt speed (greater than 300 ft/min or 1.52 m/s) before completing the test and generating the report.

   To make sure the box stays level to the belt, add weight to the box. Give the box enough distance before the tunnel, so it moves through at full speed.

   To see the passed test details, follow the same steps as in Right-Justified Test.

   To proceed to the Result Summary step, click on Next Step.

7. In the Result Summary step you can review the summary of the dynamic tests.

   When you click on Next Step, the Complete Dynamic Test pop-up appears.

   To complete the dynamic test and switch to the next step, click on Confirm.

   Note: If you have to abort the test at any time, you can click on the Cancel button at the bottom of the page.

8. The Restore & Report step restores devices to their original settings. Additionally, a report of the dynamic test results is also available for downloading.

   To download the test report, click on Download Report. Fill in the details in Generate Dynamic Test Report pop-up, and click on Generate Report.

   The report generation is complete and the file opens up.