# MQTT Forwarding

The MQTT Forwarding page of the Settings application allows you to set up network connections for forwarding to the IoT devices. You can configure MQTT, SSL/TLS, Sparkplug, and AWS settings on the MQTT Forwarding page.

You can also upload certificates, private keys, or bundles using the buttons at the top. It is possible to upload a .crt, .csr, .pem, or .key file.

By enabling Send Standard DataMan Results and Send DataMan Statistics, you send results and statistics from the DataMan devices.​

You can select readers to forward data from under DataMan Readers.

To implement any changes you make, click Save.

See below about the forwarded data for Standard DataMan Results and DataMan Statistics:

Standard DataMan Results | DataMan Statistics​ ​
--- | ---
Decode Results​ Decode Time ​ Image Index​ Is Good Read ​ Module Size​ ​ | Read Setup Index ​ Read String ​ Result Index​ Source Device Mac Address ​ Source Device Name​ Device Mac Address​ Encoder End Tick ​ Encoder Start Tick​ Group​ Timestamp​ Trigger End Time ​ Trigger Index​ Trigger Start Time​ Trigger Time ​ Unique Id​ ​ | Good Read Count No read Count​ Passed Validation Count​ Failed Validation Count​ Buffer Overflow Count​ Missed Trigger Count​ Trigger Overrun Count​ Timestamp​ Device Mac Address​
Symbology​ Angle​ Center​ Id​ Name​ Size​
Process Control Metrics ​ Standard​
Validation Error Code​ Error Position ​ Error Text​ Is Read String Valid​ ​