# Edge Intelligence

The Edge Intelligence settings page shows the network configuration, and allows you to edit and save the network settings of the EI Tunnel Manager device.

Section | Item | Description
--- | --- | ---
Network Configuration | Hostname | The hostname of the EI Tunnel Manager.
Enable DHCP | Toggle the switch to enable using DHCP protocols instead of static protocols.
IP Address | The IP Address of the EI Tunnel Manager.
Subnet Mask | The Subnet Mask of the EI Tunnel Manager. Note: Do not set more than one network port to the same subnet mask.
Gateway | The Gateway of the EI Tunnel Manager.
DNS Server | The DNS server of the EI Tunnel Manager.
Network Address Translation (NAT) | Toggle the switch to enable the NAT. See Setting up the NAT.
Clear Databases | Clear the device lists, data, and images from the EI Tunnel Manager, and create a new state. Note: The Clear database option is only available with Admin level clearance.
Reboot Edge Intelligence | Reboot the EI Tunnel Manager device.
Set Date & Time using Network Time Protocol (NTP) server | Add an NTP server to set the system time: Click +. Enter the IP address of the NTP Server. Click Save. Note: You need to log out and log back in after saving the system time.
Manual Date & Time | Toggle Set Date & Time Manually to specify the date, time and the time zone. Note: You need to log out and log back in after saving the system time.
Edge Intelligence as local NTP server | Toggle the switch to synchronize the date and time of your devices with the Edge Intelligence.