# DataMan

The DataMan page of the Provisioning app provides a list of standalone readers, as well as reader groups, and allows you configure what data you want to collect from each of your readers. You can also provision one or more of your readers at the same time, or individually by IP address.

To refresh the list of connected readers, click Refresh in the header.

To provision readers, click Provision devices and use the pop-up dialog to select the readers. To provision a reader by IP address, click Provision device by IP and enter the reader IP address.

Click Save to apply any changes you make to data collection settings.

## Actions

You can perform actions on an individual reader by clicking on the icons in the Actions column of the row for the selected reader:

Icon | Action
--- | ---
| Flash LED
| Delete

- Click the Flash LED button to remotely trigger the LED of the reader for easy identification.
- Click the Delete button to remove the reader from the list.

## Provisioning Devices

Click on Provision devices in the header to open the Provision devices pop-up dialog:

The Provision devices dialog provides a list of connected readers. To provision one or more readers, check the checkbox for the selected readers, and click Provision.

To flash the LED on a reader for easier identification, click the Flash LED icon in the Action column of the row for the selected reader.

To refresh the list of connected readers, click Discover Devices.

To search for a specific reader in the list, enter the name or IP address in the Search bar.

## Provision Device by IP

Click on Provision device by IP in the header to open the Provision device by IP pop-up dialog:

Enter the IP address of the selected reader, and click Provision.

## Data Collection Settings

You can modify collection settings for different types of data using the toggles in each column of the row for the selected reader:

Column | Description
--- | ---
Password | Provide the password for the reader to make any changes.
Collect Good Read Triggers | Enable this setting to collect good read trigger data from the reader.
Collect No Read Triggers | Enable this setting to collect no read trigger data from the reader.
Collect Validation Failure Triggers | Enable this setting to collect validation failure trigger data from the reader.
Collect Good Read Images | Enable this setting to collect good read image data from the reader.
Collect No Read Images | Enable this setting to collect no read image data from the reader.
Collect Validation Failure Images | Enable this setting to collect validation failure image data from the reader.
Collect Device Configuration Changes | Enable this setting to collect reader configuration change data from the reader.
Collect Statistics | Enable this setting to collect statistics from the reader.
Collect Tunnel Trigger Result | Enable this setting to collect tunnel trigger results from the reader.

To order the list of readers by type of data collection enabled, click on a data collection column header.