# Stitcher Settings

The Stitcher feature stitches images together into one bigger image. The stitched images appear in the Results Browser as normal images.

Note: Only the EI-A9-TUNMGR-xxx hardware supports image stitching.

Number | Description
1 | Click the Stitcher Enabled checkbox to enable the type. You can choose the type of the Stitcher feature: Modular Vision Tunnel (MVT): A flexible scan tunnel in which the units can detect up to six sides of the boxes. Scalable for various speeds and gaps, without sacrificing accuracy. Top Only No Perspective: For units that only aimed at the top of the boxes.
2 | Choose the image format from the dropdown: JPG PNG BMP Choose the image size from the following: Full Quarter 1/16 1/64
3 | Adjust the quality of the output image on the slider or write a number in the box. Select the Dots per Inch (DPI) value of the output images for each trigger type: 100 DPI: lower quality, suitable for long-term storage and basic analysis. 150 DPI: sacrifice some quality to reduce storage size. 210 DPI: suitable for post-processing, for example OCR. Do not stitch: you can choose not stitching the images together for that particular trigger type.
4 | Select the Multi-Reader Sync (MRS) group. You can choose a group if there are multiple groups provisioned on the Edge Intelligence system.
5 | Select which sides of the boxes you want to stitch into one image. For example, if you have a unit that detects the top and the front of a box, you can select only the top to be stitched into one image.