# Specifications

Category | Specification
EI-A3 Series | EI-A9 Series
Standard Color | Silver and black
Construction | Aluminum extrusion heavy-duty cold-rolled steel
Processor | Intel® 13th generation Core™ i3-13100T (35 W, 2.1 GHz performance core base frequency) | Intel® 12th generation Core™ i9-12900TE (35 W, 2.5 GHz performance core base frequency)
Note: The IPC might cause CPU frequency hopping when operating in an extremely high temperature environment. Thermal throttling can occur when the system remains in full loading conditions. The performance of the system might be adversely affected when operating at a temperature above the limitation of the system.
Memory | 8 GB | 16 GB
Ethernet | 2 × 2.5 GbE LAN (Intel® I226-V, M12 X-coded) 1 × 1 GbE LAN (Intel® I219-LM, M12 X-coded)
USB | 4 × USB3.2 Gen1x1 (5G) type A
Display | 1 × HDMI 1.4b with 4096 × 2160 resolution supported
TPM | 1 × TPM 2.0 on board
Storage | 256 GB M.2 SSD, wide temperature | 1 TB M.2 SSD, wide temperature
Power input | DC input: 24 V DC (±5%), 16 A, M12 (L-coded, male, 5-pin), 2.1 A typical maximum load, without accessories 3 A power supply capacity recommended | DC input: 24 V DC (±5%), 16 A, M12 (L-coded, male, 5-pin), 5 A typical load with 8 A spikes, without accessories 8 A power supply capacity recommended
DC output: 24 V DC (±5%), 11 A, M12 (L-coded, female, 4-pin), 11 A maximum pass-through current, when using sufficiently-rated power supply 1 x power switch with LED
Typical | 24 V DC
Power rating | 24 V DC, 16 A Note: The system power rating might change based on differing combinations of attached devices.
Operating Temperature | -20 °C to 40 °C, with 10% to 95% non-condensing relative humidity. Includes an industrial wide-temperature SSD and requires 0.7 m/s air flow
Storage Temperature | -40 °C to 70 °C, with 10% to 95% non-condensing relative humidity
IP Rating | IP54
Vibration | Operational: 3 Grms, 2 hr/axis, 10-500 Hz Shipment: 2.25 Grms, 2 hr/axis, 10-500 Hz
Shock | IEC 60068-2-27 (with SSD: 50G, half sine, 11 ms duration)
Dimensions | 270 × 255 × 86.5 mm (including embedded wall mount)
Weight (net/gross) | 4.8 kg/5.5 kg
Regulations/Conformity | CE, FCC, UL, CB, KC, CCC, BIS, VCCI Note: For more information, see Regulations and Conformity.