# Connecting the Network and Power Cables

To connect the network and power cables:

1. Unpack your Edge Intelligence unit and ensure all components are included.

2. Connect the Edge Intelligence unit to your production network.

   1. Connect to your network using Ethernet port 1 or 3.

   2. Connect to your reader or vision system network LAN using Ethernet port 2.

   Number | Port
   --- | ---
   1 | 1 GbE external port (DHCP)
   2 | 2.5 GbE internal port (192.168.1.100)
   3 | 2.5 GbE internal port (DHCP default)

3. Connect the Edge Intelligence unit to a power source, using port 1 for power input and port 2 for power output.

   Number | Port
   --- | ---
   1 | DC input: 24 V DC(±5%), M12 (L-coded, male, 5-pin) 4 A typical load, without accessories 16 A maximum input current
   2 | DC output: 24 V DC (±5%), M12 (L-coded, female, 4-pin) 11 A maximum pass-through current, when using sufficiently-rated power supply