# Hybrid Switches

The Hybrid Switches page of the Device Management app allows you to manage hybrid switches.

Item | Description
--- | ---
Action ribbon | Provides quick access to actions you can perform on the selected switches.
Button | Description
--- | ---
Upload Firmware | Upgrade firmware on selected switches.
Discover Devices | Find switches on the local and remote networks, depending on the configuration on the Remote Subnets page.
Device list | A table view of the settings of the switches that are discovered on the network with options that can be enabled or disabled for the switch.

## Columns of the Table View

The table view of the switches displays information and allows setting changes to the individual switches.

Column Title | Description
Actions | Click on the icons to perform actions on an individual switch.
Icon | Button Name | Description
| Edit Switch Network Settings | Modify the name, IP address, Subnet Mask, and Default Gateway of the switch.
| Flash LED | Remotely trigger the LED of the switch for easy identification.
| Open WebHMI | Opens the WebHMI in a pop-up window. For more information, see the WebHMI Window section in this topic. Note: When you connect directly to the EI Tunnel Manager using a monitor, the Open WebHMI button is not available.
Name | A customizable name of the switch.
MAC Address | The MAC address of the switch.
Firmware Version | The version of firmware installed on the switch.
Address Type | Indicates network address type (DHCP or static) for the switch.
IP Address | The IP address of the switch.
Subnet Mask | The subnet mask of the switch.
Gateway | The gateway of the switch.
Source Network Interface | The Ethernet port the switch uses for connection.
State | Displays the state of the switch, which can be: In Local Subnet In Remote Subnet In Remote Subnet Behind NAT Waiting For DHCP Misconfigured Unknown