# Estimate Runtime Performance

The following numbers are an approximate guide to the potential runtime performance increment for different card families (baseline = non-TensorCore, standard mode):

ViDi operating mode | No Tensor Cores (example GTX) | Volta Tensor Cores (example V100) | Turing Tensor Cores (example T4)
--- | --- | --- | ---
Standard | 100% | 150% | 150%
Low Precision | 125% | 125% | 175%

Note: In comparison with other Tesla cards, the T4 is oriented toward runtime operation. It supports ViDi training and runtime, but training performance will likely be slower than a V100.