# Working with Non-square Pixels

If your camera has non-square pixels and your application requires high-accuracy location of rotated patterns, you must calibrate your system and apply the calibration to run-time images and to training images when training from an image. When using shape descriptions, the shapes should be specified in the calibrated space, and the calibrated space should be the selected space of each run-time image.